The following is additional information regarding Invitation to Bid SPU 3700, **Solids and Liquids Waste Disposal** Released on 03/07/2017. **The due date and time for** **responses remains as 03/30/2017; 4:00PM** (Pacific). This addendum includes both questions from prospective bidders and the City’s answers, and revisions to the bid. This addendum is hereby made part of the ITB and therefore, the information contained herein shall be taken into consideration when preparing and submitting a proposal.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Item # | Date Received | Date Answered | Vendor’s Question | City’s Answer | ITB Revisions |
| 1 | 3/20/2017 | 3/23/2017 | SEWER GRIT- SPU-  How is SPU currently disposing of this sanitary sewer grit waste?  | After a decanting process, SPU sewer grit solids are transported to a local transfer station under an approved profile for landfill disposal. When local transfer stations are temporarily shut-down due to rail issues, the sewer grit solids are direct hauled to King County Cedar Hills, under a separate temporary waste clearance provision. |  |
| 2 | 3/20/2017 | 3/23/2017 | SEWER LIQUIDS- CITY LIGHT- How is City Light currently disposing of this sanitary liquids?  | City Light sanitary liquids are removed via vactor companies who have their own decant and disposal options. |  |
| 3 | 3/20/2017 | 3/23/2017 | Sewer Grit: Will the waste be treated to kill pathogens, Bleach, Cleaners, prior to arrival at disposal facility?  | The Sewer grit waste is not treated. The waste stream is tested for waste characterization and receiving facility profile acceptance.   |  |
| 4 | 3/20/2017 | 3/23/2017 | Sewer Liquids: Will the liquids be  treated to kill pathogens, Bleach, Cleaners, prior to arrival at disposal facility? | The sewer liquid waste is not treated.  |  |
| 5 | 3/20/2017 | 3/23/2017 | Drum disposal pricing should be by per drum rate for disposal for each solidification then landfill and solids for direct landfill.  Cubic Yard containers could be factored at 3.4 times the drum rate.   | That is acceptable.  |  |
| 6 | 3/20/2017 | 3/23/2017 | Drum transport could best be factored by 0-10 drums with minimum stop fee, 10-30 drums, Likely used for small projects or Investigative Derived waste (IDW).   | That is acceptable. |  |
| 7 | None | 3/23/17 | The City has made the following edits to the specification found on page 3 of 14 in order to address those SCL locations outside of the Greater Seattle area. | Please see revisions to the ITB specifications in mark up. |  |
| 8 | None | 3/23/17 | The City has made the following edits to the background statement on page 2 of the Invitation to Bid.  | Please see revision to the ITB background statement.  | Originally published as:**Background:** Currently we have contracts with three vendors and the City is returning to the marketplace for a competitive bid to establish new contract(s). We estimate that we currently produce approximately 5000 tons of waste per year. Over the past year the City has spent nearly $293,000 dollars on vactor waste. The primary users of this service are: Seattle Public Utilities, Seattle City Light, Parks Department, and Seattle Department of Transportation. Will now be revised to read:**Background:** Currently we have contracts with three vendors and the City is returning to the marketplace for a competitive bid to establish new contract(s). We estimate that we currently produce approximately ***65,000*** tons of waste per year. Over the past year the City has spent nearly $293,000 dollars on vactor waste. The primary users of this service are: Seattle Public Utilities, Seattle City Light, Parks Department, and Seattle Department of Transportation.  |