The following is additional information regarding Invitation to Bid/Request for Proposal # SC0-23 titled Audio System for Seattle Center Mural Upgrade released on 02/05/2019. **The due date and time for responses has been changed to 03/07/2019; 3:00PM (Pacific)**. This addendum includes both questions from prospective proposers and the City’s answers and revisions to the ITB. This addendum is hereby made part of the ITB and therefore, the information contained herein shall be taken into consideration when preparing and submitting a bid.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Item # | Date Received | Date Answered | Vendor’s Question | City’s Answer | RFP Revisions |
| 1 | 02/12/2019 | 02/12/2019 | **City Initiated – Rescheduled Pre-Bid and Revised bid due date** |  | Due to the recent inclement weather we have experienced, the schedule has been revised as follows: See Page 1, Table 1: Solicitation Schedule. Revise to read:  Pre-Bid Conference (Optional) - 02/20/2019; 3:00PM  Deadline for Questions – 02/22/219  Sealed Bids Due to the City – 03/07/2019; 3:00PM |
| 2 | 02/12/2019 | 02/13/2019 | **City Initiated – Revised Adamson S-10 Speaker configuration** | . | See Page 3, Section 5: Specifications and Scope of Work. Revise 2.2 SPEAKER CABINETS and CONTROL to read: six S10 speakers and six S10N speakers.  <https://www.adamsonsystems.com/en/product/s-series/s10n>  See Page 11, Section 7, Item 4 Bid Offer Form: Line 1 Adamson S10 Line Array Cabinet revise Qty to 6. Add line item for S10N speakers Qty 6 |
|  | 02/15/2019 | 02/22/2019 | Item 2 Adamson S19 Subwoofer NL4. The model number should read S119, not S19 |  | Correct, Adamson S119 Subwoofer <https://adamsonsystems.com/Support/Downloads/SPEC_SHEETS/S_SERIES/S119_Technical_Data.pdf> |
| 4 | 02/15/2019 | 02/22/2019 | Item 6 Olympic Case 12RU Fastrack amp rack; how deep does the case need to be? Please give us measurement from rail to rail or cover to cover. | <http://olycase.com/2016/10/fastpack-rack/>  Olympic Case Company Fastpack Shockmount Racks. The rack must be deep enough to fit a Lab Gruppen D80:4L Amplifier which is 18-1/2” from rack ears to rear edge. We also want each rack to have an internal sleeve shockmounted inside the main rack case. |  |
| 5 | 02/15/2019 | 02/22/2019 | Item 6 Olympic Case 12RU Fastrack amp rack, do you need casters? | Yes |  |
| 6 | 02/15/2019 | 02/22/2019 | Item 6 Olympic Case 12RU Fastrack amp rack, what color would you like the case to be? | Black,  <http://olycase.com/wp-content/uploads/2016/01/10865064_1386782338284810_352148682_n.jpg> |  |
| 7 | 02/15/2019 | 0222/2019/ | Item 14 TBD 12 Space Rack. We need more specifics on the rack please: front and rear rails, doors, shelves, screws, blank panels, casters??? Is there a preferred vendor? | Same Olympic Fastpack rack case as described above  <http://olycase.com/fastpack-cases/> |  |
| 8 | 02/20/2019 | 02/22/2019 | Question on Section 5, Specification and Scope of Work, Page 4, Prohibition on Advance Payments  Adamson Speakers has a vendor payment policy of 50% down payment with order, balance due prior to shipment. These terms are noted on the MSRP quote from Adamson attached.  In light of this, is there something the City is able to do to work with the winning bidder on this to mitigate the bidder having to float the cost ($100K plus) of the Adamson (and other) products for 60 days?  The 60-day calculation is based upon their normal lead time ARO at 3-4 weeks and shipping time from Canada at a week. Once we invoice then City of Seattle terms are I believe Net 30? |  | The City will negotiate progress payment terms with the successful bidder to address the Manufacturers payment policy to mitigate the successful bidders float. |
| 9 | 02/22/2019 | 02/25/2019 | It appears that the model # for the cable is off at the end by one letter. It should read PC224T for standard application or TC224TP for Plenum application.  <http://pub.tmb.com/ProPlex/DataCables/pdf/ProPlexT-LTR-web.pdf> |  | Revise model # for cable to read PC224T. |
| 10 |  |  |  |  |  |
| 11 |  |  |  |  |  |